= gpscsv(1)
:author: Gary E. Miller
:date: 28 July 2021
:email: gem@rellim.com.
:keywords: gps, gpsd, gpscsv, csv
:manmanual: GPSD Documentation
:mansource: GPSD, Version {gpsdver}
:robots: index,follow
:sectlinks:
:toc: macro
:type: manpage

include::../www/inc-menu.adoc[]

== NAME

gpscsv - dump the JSON output from gpsd as CSV

== SYNOPSIS

*gpscsv* [OPTIONS] [host[:port[:device]]]

*gpscsv* -h

*gpscsv* -V

== DESCRIPTION

*gpscsv* is a simple Python program for reading *gpsd* JSON data streams
and outputting them in Comma Separated Values (CSV) format. It takes
input from a specified *gpsd* and reports to standard output. The program
runs until the *gpsd* dies, "*-n COUNT*" messages are processed,
"*-x SECONDS*" have passed, or it is interrupted by ^C or other means.

*gpscsv* can only collect data that your *gpsd* is already sending.  Use
*gpspipe* to see what JSON message classes it is sending.

One good use of *gpscsv* is to create CSV files for use with the gnuplot
program.

*gpscsv* does not need root, but will run fine as root.

== OPTIONS

The program accepts the following options:

*-?*, *-h*, *--help*::
  Show help information and exit.
*-c MCLASS*, *--class MCLASS*::
  Select the JSON class messages of type MCLASS. Overrides the default
  class of TPV.  See the <<Classes>> section below for more information.
*--cvt-isotime*::
  Convert fields named "time" from ISO time to UNIX time.
*-D LVL*, *--debug LVL*::
  Set debug level to LVL. Default 0. Higher arguments than 0 produce
  more debug output.
*--device DEVICE*::
  The DEVICE on the *gpsd* to connect to. Defaults to all.
*-f FIELDS*, *-fields FIELDS*::
  The FIELDS from the JSON message to dump to the output. Set FIELD to
  empty ('') for all initially seen fields. Default varies by CLASS.
*--file FILE*::
  Read JSON from FILE instead of from *gpsd*.
*--header HEADER*::
  Set header style to HEADER. 0 for no header, 1 output fields as
  header, 2 send fields as a comment ('#'). Defaults to 1.
*--host HOST*::
  Connect to the *gpsd* on HOST. Defaults to localhost.
*-n COUNT*, *--count COUNT*::
  Exit after outputting COUNT records. Set COUNT to 0 to disable.
  Default is 0
*--port PORT*::
  Use PORT to connect to *gpsd*. Defaults to 2947.
*--separator SEPARATOR*::
  Use SEPARATOR as the field separator. Default separator is a comma
  (',').
*-V*, *--version*::
  Show *gpscsv* version, and exit.
*-x SECONDS*, *--seconds SECONDS*::
  Exit after SECONDS number of seconds have passed. Set SECONDS to 0 to
  disable. Default is 0

All the above individual options may be specified multiple times, but  t
only the last one off each will be used.

== Classes

Some of the *gpsd* JSON message classes include sub-classes.  *gpscsv*
allows direct access to them using a meta-class (MCLASS).

|===
|MCLASS |Class |Description

|ALMANAC |SUBFRAME | ALMANAC from SUBFRAME JSON
|HEALTH |SUBFRAME | HEALTH from SUBFRAME JSON
|HEALTH2 |SUBFRAME | HEALTH2 from SUBFRAME JSON
|IONO |SUBFRAME | IONO from SUBFRAME JSON
|NMCT |SUBFRAME | NMCT from SUBFRAME JSON
|SUBFRAME1 |SUBFRAME | SUBFRAME1 (Ephemeris 1) from SUBFRAME JSON
|SUBFRAME2 |SUBFRAME | SUBFRAME2 (Ephemeris 2) from SUBFRAME JSON
|SUBFRAME3 |SUBFRAME | SUBFRAME3 (Ephemeris 3) from SUBFRAME JSON
|SAT |SKY | Individual satellites from SKY
|SKY |SKY | The basic parts of SKY JSON
|TPV |TPV | The basic parts of TPV JSON

|===

== ARGUMENTS

By default, clients collect data from the local *gpsd* daemon running
on localhost, using the default GPSD port 2947. The optional argument
to any client may override this behavior: *[server[:port[:device]]]*

For further explanation, and examples, see the *ARGUMENTS* section in
the *gps*(1) man page

== EXAMPLES

Some basic standalone examples:

Grab three cycles of TPV data:

----
$ gpscsv -c TPV -n 3
time,lat,lon,altHAE
2021-07-28T22:38:37.000Z,44.0688638,-121.3140643,1108.223
2021-07-26T22:38:37.000Z,44.068863833,-121.314064333,1108.3
2021-07-28T22:38:38.000Z,44.0688637,-121.314065,1108.363
----

Grab one set of satellite data:

----
$ gpscsv -c SAT -n 1
time,gnssid,svid,PRN,az,el,ss,used,health
2021-07-28T22:37:46.000Z,0,8,8,311.0,28.0,33.0,True,1
2021-07-28T22:37:46.000Z,0,10,10,290.0,74.0,50.0,True,1
2021-07-28T22:37:46.000Z,0,15,15,45.0,18.0,31.0,False,1
2021-07-28T22:37:46.000Z,0,16,16,244.0,7.0,23.0,True,1
2021-07-28T22:37:46.000Z,0,18,18,109.0,43.0,37.0,True,1
2021-07-28T22:37:46.000Z,0,23,23,49.0,62.0,38.0,True,1
2021-07-28T22:37:46.000Z,0,24,24,87.0,16.0,28.0,True,1
2021-07-28T22:37:46.000Z,0,27,27,280.0,52.0,42.0,True,1
2021-07-28T22:37:46.000Z,0,32,32,188.0,32.0,42.0,True,1
2021-07-28T22:37:46.000Z,5,3,195,305.0,6.0,13.0,False,1
2021-07-28T22:37:46.000Z,6,2,66,38.0,8.0,21.0,False,1
2021-07-28T22:37:46.000Z,6,3,67,34.0,60.0,32.0,True,1
2021-07-28T22:37:46.000Z,6,4,68,226.0,63.0,34.0,True,1
2021-07-28T22:37:46.000Z,6,5,69,220.0,12.0,32.0,True,1
2021-07-28T22:37:46.000Z,6,11,75,-999,4.0,0.0,False,2
2021-07-28T22:37:46.000Z,6,12,76,47.0,0.0,0.0,False,1
2021-07-28T22:37:46.000Z,6,17,81,142.0,8.0,31.0,True,1
2021-07-28T22:37:46.000Z,6,18,82,138.0,57.0,40.0,True,1
2021-07-28T22:37:46.000Z,6,19,83,333.0,70.0,29.0,True,1
2021-07-28T22:37:46.000Z,6,20,84,323.0,10.0,0.0,False,1
----

=== Plot Examples

Some plot examples, do them in exact order shown:

Grab 100 samples of time,lat,lon,altHAE:

----
  $ gpscsv -n 100 --cvt-isotime  > tpv.dat
----

Grab 100 samples of time,epx,epy,epv,eph,sep

----
  $ gpscsv -n 100 --cvt-isotime -f time,epx,epy,epv,eph,sep > ep.dat
----

Grab 100 samples of time,xdop,ydop,vdop,tdop,hdop,gdop,pdop

----
  $ gpscsv -n 100 --cvt-isotime -c SKY  > sky.dat
----

Grab 100 samples of time,nSat,uSat

----
  $ gpscsv -n 100 --cvt-isotime -c SKY -f time,nSat,uSat  > sat.dat
----

=== Viewing CSV data with gnuplot

Start gnuplot in interactive mode:

----
  $ gnuplot
----

Some gnuplot housekeeping:

----
  # this are csv files
  gnuplot> set datafile separator ','
  # use the first line as title
  gnuplot> set key autotitle columnhead
  # X axis is UNIT time in seconds.
  gnuplot> set xdata time
  gnuplot> set timefmt "%s"
----

Now to plot time vs latitude, using *tpv.dat* from above:

----
  gnuplot> plot 'tpv.dat' using 1:2
----

Then to plot longitude and altHAE, in separate plots:

----
  gnuplot> plot 'tpv.dat' using 1:3
  gnuplot> plot 'tpv.dat' using 1:4
----

Put both latitude and longitude on one plot:

----
  gnuplot> set y2tics
  gnuplot> plot 'tpv.dat' using 1:2, '' using 1:3 axes x1y2
----

Plot epx, epy, epv, eph, and sep in one plot, using *ep.dat* from above:

----
  gnuplot> plot 'ep.dat' using 1:2, '' using 1:3, \
           '' using 1:4, '' using 1:5, '' using 1:6
----

Plot all the DOPs on one plot, from *sky.dat* above:

----
  gnuplot> plot 'sky.dat' using 1:2, '' using 1:3, '' using 1:4, \
           '' using 1:5, '' using 1:6, '' using 1:7, '' using 1:8
----

Plot nSat and uSat together:

----
  gnuplot> plot 'sat.dat' using 1:2, '' using 1:3
----

Lat/lon scatter plot:

----
  # x is no longer time
  gnuplot> set xdata
  gnuplot> plot 'tpv.dat' using 3:2 title 'fix'
----

== RETURN VALUES

*0*:: on success.
*1*:: on failure

== SEE ALSO

*gpspipe*(1), *gpsd_json*(5), *gpsd*(8), *gnuplot*(1)

== RESOURCES

*Project web site:* {gpsdweb}

== COPYING

This file is Copyright 2020 by the GPSD project +
SPDX-License-Identifier: BSD-2-clause
