= gpssnmp(1)
:date: 18 May 2024
:keywords: gps, gpsd, gpssnmp
:manmanual: GPSD Documentation
:mansource: GPSD Version {gpsdver}
:robots: index,follow
:sectlinks:
:toc: macro
:type: manpage

include::../www/inc-menu.adoc[]

== NAME

gpssnmp - SNMP helper client for gpsd

== SYNOPSIS

*gpssnmp* [OPTIONS] [server[:port[:device]]]

*gpssnmp* -h

*gpssnmp* -g OID

*gpssnmp* -n OID

*gpssnmp* -p

*gpssnmp* -V

== DESCRIPTION

*gpssnmp* is a *gpsd* client that works as an SNMP helper for *MRTG*.

*gpssnmp* does not require root privileges. It will also run fine as root.

*gpssnmp* can act as an agent to *snmpd* in _pass_ mode or in
_pass_persist_ mode. So it can be used to extend *snmpd* with the
*GPSD-MIB*.  Given the nature of the *SNMP* protocol, do not expect
good latency.  Data from different epochs may be mixed up together.

NOTE: this program is new in version 3.24.1 and will be subject to
change for a few revisions.  Consider it a Work In Progress (WIP).

== OPTIONS

*-?*, *-h*, *--help*::
  Print a summary of options and then exit.
  Use with "-D 1" to see valid OID values.
  Use with "-D 2" to see valid OID values with scale values and descriptions.
*-g OID*::
  Get the specified OID.
*-n OID*::
  Get the next OID starting at OID.
*-p*, *--persist*::
  Enter _pass_persist_ mode.  This allows better performance when used as
  an agent for the *snmpd* daemon.  See the snmpd.conf man page for details.
*-V*, *--version*::
  Print the package version and exit.


== EXAMPLES:

To get the number of saltellits seen with the OID

----
   $ gpssnmp -g .1.3.6.1.4.1.59054.11.2.1.3.1
   .1.3.6.1.4.1.59054.11.2.1.3.1
   INTEGER
   15
----

To get the number of saltellits seen with the MIB name

----
   $ gpssnmp -g skynSat.1
   .1.3.6.1.4.1.59054.11.2.1.3.1
   INTEGER
   15
----

=== Connecting to snmpd

*gpssnmp* can work as a "pass-through script" with *snmpd*.  To enable
this functionality on an already working snmpd installation, add this to your
*snmpd.conf* file, and then restart *snmpd*:

----
# be sure SNMPv2 community "public" can access all MIBs:
rocommunity public  localhost

# configure pass-through of GPSD-MIB to gpssnmp
pass .1.3.6.1.4.1.59054  /usr/local/bin/gpssnmp
----

You can then query the number of satlettites in use this way:

----
$ snmpget -c public -v 2c localhost skynSat.1
GPSD-MIB::skynSat.1 = INTEGER: 16
----

Dump the entire "sky" OID this way:

----
$ snmpwalk -c public -v 2c localhost GPSD-MIB::sky
GPSD-MIB::skynSat.1 = INTEGER: 17
GPSD-MIB::skyuSat.1 = INTEGER: 8
GPSD-MIB::skySNRavg.1 = INTEGER: 2000
----

Dump the entire GPSD-MIB this way:

----
$ snmpwalk -c public -v 2c localhost gpsd
GPSD-MIB::tpvLeapSeconds = INTEGER: 18
GPSD-MIB::tpvNumber = INTEGER: 1
GPSD-MIB::tpvIndex.1 = INTEGER: 1
[...]
----

*gpssnmp* supports the _pass_persist_ mode of snmpd.  To have
*snmpd* use *gpssnmp* in this mode put this in your _snmpd.conf_
file:

----
pass_persist .1.3.6.1.4.1.59054  /usr/local/bin/gpssnmp --persist
----

== RETURN VALUES

*0*:: on success.
*1*:: on failure

== SEE ALSO

*cgps*(1), *gps*(1), *gpspipe*(1), *snmpget*(1), *snmpwalk*(1), *xgps*(1)

*snmpd.conf*(5)

*gpsd*(8), *snmpd*(8)

== RESOURCES

*Project web site:* {gpsdweb}

== COPYING

SPDX-FileCopyrightText: The GPSD project +
SPDX-FileType: DOCUMENTATION +
SPDX-License-Identifier: BSD-2-clause 
